;basp.ldi
;Broadcom Corp  
;VeRsIoN=1.00 Novell LAN Installation Information File for BASP.
;CoPyRiGhT=(c) Copyright 2000,2001,2002,2003 by Broadcom Corporation. All rights reserved.

VER:    1.00
SYN:    1.00

DR LB_1
{
	DESC:   $bcm_1
	PAR:    2.00
	FILE:   BASP.LAN
	OFILE:	BMAPI.NLM
	OFILE:	BSNMP.NLM
	PROD:   'EISA.ISA.871.2'

        ;@#  SPROD 'Broadcom~ Virtual Adapter'

        ;@#  Client:basp
        ;@#  Alias:basp.lan

   PR VSLOT REQUIRED
   {
        DES:        "Virtual Slot for this virtual adapter"
        TYPE:       DECIMAL(1)
        VAL:        1-4
        Default:    1
    	OutputFormat:  'VSLOT=%s'
   }

   LIST MODE OPT
   {
	DES: $bcm_11

	HELP: $bcm_12 

	CD: $bcm_13 
	CH: $bcm_14 
	
	CD: $bcm_15 
	CH: $bcm_16 
	
	CD: $bcm_17 
	CH: $bcm_18 
	
	Default: 1
    	OutputFormat:  'MODE=%s'
   }

   PR VLAN OPT
   {
        DES:        "VLAN ID"
        TYPE:       DECIMAL(4)
        VAL:        0-4095
        Default:    0
    	OutputFormat:  'VLAN=%s'
   }

   FR	FrameSelect
   {

	DES:	$bcm_5
	HELP:	$bcm_6

	CD:	$bcm_7
	CH:	'Ethernet_802.2'

	CD:	$bcm_8
	CH:	'Ethernet_802.3'

	CD:	$bcm_9
	CH:	'Ethernet_SNAP'

	CD:	$bcm_10
	CH:	'Ethernet_II'

	Default: 4
   }
}



DLANG:	4
;English
	$bcm_1 = "Broadcom Virtual Adapter "
	$bcm_5 = "Frame Types"
	$bcm_6 = "Select a frame."
	$bcm_7 = "802.2"
	$bcm_8 = "802.3"
	$bcm_9 = "802.2 SNAP"
	$bcm_10 = "Ethernet II"
	$bcm_11 = "Balance Mode"
	$bcm_12 = "Smart Load Balance (SLB) is default. Choose Generic Trunk (TRUNK) or IEEE 802.3AD if switch support these modes."
	$bcm_13 = "Smart Load Balance"
	$bcm_14 = "SLB"
	$bcm_15 = "Generic Trunking"
	$bcm_16 = "TRUNK"
	$bcm_17 = "IEEE 802.3AD"
	$bcm_18 = "802.3AD"
