� StorageWorks and the DIGITAL logo are trademarks of Digital Equipment Corporation. EK ˘ 35XEC ˘ IG .B01

©Digital Equipment Corporation 1997 June 1997

Printed in the U.S.A.

All Rights Reserved.

DIGITAL StorageWorks

PVA Installation Guide

This guide describes the procedures for removing and

installing an ultra SCSI RAID subsystem power verification

and addressing (PVA) assembly, model DS ˘ BA35X ˘ EC.

Removing and installing a PVA requires completing the

following actions:

1. Shut down the controller as described in the latest version

            of the DIGITAL StorageWorks HSZ70 Array Controller

            HSOF Version 7.0 Service Manual .

2. Turn off enclosure power using the ac power input

            switches.

3. Remove and replace defective PVA.

4. Apply power to the enclosure.

5. Start the controller as described in DIGITAL

            StorageWorks HSZ70 Array Controller HSOF Version 7.0

            Service Manual .

              ____________ CAUTION ________________

                 To protect this sensitive electronic device from

                 electrostatic discharge (ESD) use the following

                 precautions ˙ (1)   Wear an ESD wrist strap.

                 (2)   Do not touch the printed circuit board or the

                 backplane connector.  (3)   Do not lay the device

                 on a work surface but place it on an electrostatic

                 mat.  (4)   Place the device in an electrostatic bag

                 for shipment.

              ________________________________ __________

              ______________ Note ___________________

                 For detailed information about the operation,

                 function, status, error conditions, fault conditions,

                 and displays of this device, refer to the  DIGITAL

                 StorageWorks Ultra SCSI RAID Enclosure User´s

                 Guide .

              ________________________________ __________

Removing a PVA

Complete the following procedure to remove a PVA from the

ultra SCSI RAID enclosure.

1. After shutting down the controller and turning

O
FF
the

enclosure power, pull the PVA extractor handles to the

front to loosen the PVA from the backplane connector.

2. Remove the PVA from the enclosure and note enclosure

device address

2 2

Installing a PVA

Complete the following procedures to install a PVA in an

ultra SCSI RAID enclosure.

1. Remove the replacement PVA from the electrostatic bag.

 Verify that the unit is the correct model by checking the

            regulatory label.

2. Insert the defective PVA in the electrostatic bag for

            shipment.

3. Set enclosure address (see Step 2, ^ Removing the PVA ~ ).

4. Align the PVA with the guides in the right -hand

            enclosure slot.

5. Insert the PVA into the slot and push it in until the

            extractor latches engage the enclosure.

6. Push the extractor latches in to firmly seat the PVA.

7. Apply power to the enclosure by turning on the AC power

            controllers.

8. Start the controller as described in DIGITAL

            StorageWorks HSZ70 Array Controller HSOF Version 7.0

            Service Manual  and verify that the subsystem is

            functioning properly.