3Com (R) Corporation
SCO OpenUnix 8 Driver
3Com 3C905B/3C905C/3C980/3C982/3C980B/3C980C Fast EtherLink PCI
10/100 Base-TX Server NICs

Basic Installation Instructions

Installation

1. Add the driver package as root

	# pkgadd -d <absolute_path_to_package>/E3J.pkg

2. Install the driver, rebuild the kernel, and reboot if necessary

	# cd /etc/inst/nd/mdi/e3bc
	# /etc/conf/bin/idinstall -M e3bc
	# /etc/conf/bin/idbuild -B
	# cd /; shutdown -g0 -y

3. Configure the interface 

	# netcfg

4. Choose "Add new LAN adapter..." and the NIC will be autodetected.
You should see information about the NIC in the middle of the screen.

5. Assuming the NIC is successfully detected, choose "Add protocol..."
and pick either TCP/IP or IPX and follow the on-screen instructions.

6. Exit netcfg.

7.  Now you should be able to ping other machines on the network.  When
you reboot, TCP/IP should automatically start running and commands such
as telnet and ftp will be available.

De-installation

1. To remove the driver, type

# pkgrm e3J

2. It will then prompt you if you would like to remove the package.  Type “yes” to continue

3. The de-installation will continue

4. To confirm that the de-installation occurred, type

	# pkginfo e3J

if nothing shows up, then the interface has been removed.